


COSHH ASSESSMENT SHEET

Date of Assessment: 24.09.24 Assessment No: CA 17 Assessor: Daniel Looney

Overall Assessment Rating of Risk [ √ ] Low [√ ] Medium [ ] High [ ]

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Work Activity:** | | | | | | | | | | | Detergent for use on motor vehicles | | | | | | | | | |
| **Persons at Risk:** | | | | User [√] Colleagues [√] Contractors [ ] Public [ ] Others **[** ] | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | |
| **Name of Hazardous Substance:** | | | | | AUTOGLYM No 19A PSV Fleetclean | | | | | | | | | | | | | | | |
| **Manufacturer (address/tele no):** | | | | | AutoGlym Works Road, Letchworth, Herts, SG6 1LU | | | | | | | | | | | | | | | |
| **SDS Version:** | | | | | 12 | | | | | | | | | | | | | | | |
| **Supplier (address/tele no):** | | | | | 01462 677766 | | | | | | | | | | | | | | | |
| **Hazard data sheet attached:** | | | | | Yes [ √ ] No [ ] | | | | | | | | | | | | | | | |
| **Description/colour:** | | | | | Green | | | | | | | | | | | | | | | |
|  | **Container size in litres/kg** | | |  | **20**  **litre/kg** | | | **10**  **litre/kg** | | | | **5 litre/kg** | | | **>litre/kg** | | **< litre/kg** | | **Other** | |
|  | (tick as appropriate) | |  |  | √ | | |  | | | |  | | |  | |  | |  | |
| **HAZARD** (tick all that apply) | | | | | | | | | | | | | | | | | | | | |
|  | Corrosive | Flammable | Oxidising | | | | Corrosive | | Toxic | | | | Environmentally damaging | |  | | Health hazard | | Compressed gas |  |
|  | Explosive (Symbol: exploding bomb) | Flammable (Symbol: flame) | Oxidising (Symbol: flame over circle) | | | | Corrosive (Symbol: Corrosion) | | Acute toxicity (Symbol: Skull and crossbones) | | | | Hazardous to the environment (Symbol: Dead tree and fish) | | Health hazard/Hazard ous to the ozone layer (Symbol: Exclamation mark) | | Serious health hazard (Symbol: health hazard) | | Gas under pressure (Symbol: Gas cylinder) |  |
|  |  |  |  | | | |  | |  | | | |  | | √ | |  | |  |  |
| **Known exposure levels:**  **W.E.L.** (where applicable) | | | | | | NA | | | | | | | | | | | | | | |
| **Likely route of entry to body:**  (tick all that apply) | | | | | | **Inhaled** | | | | **Ingested** | | | | **Absorbed by skin** | | **Eyes** | | **Other** | | |
|  | | | | | |  | | | |  | | | |  | | √ | |  | | |
| **Areas of use/exposure:** | | | | | | **Bus washes** | | | | | | | | | | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **CONTROL MEASURES** | | | |
| **Can the exposure/use be eliminated or substituted?** | (tick as appropriate) | **Yes** | **No** √ |



**PERSONAL PROTECTIVE EQUIPMENT REQUIREMENT.** (tick as appropriate)

**Hard Hats**

**Face Protection**

**Eye Protection:** √

**Dust Mask**

**Respirator**

**Ear Protection**

**Overalls**

**Apron**

**Foot Protection**

**Gloves:** √

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Is monitoring required?** | (tick as appropriate) | | | **Yes** | | **No** √ | |
| **Local exhaust ventilation required?** | (tick as appropriate) | | | **Yes** | | **No** √ | |
| **Documented working method available on safe use and**  **handling?** | (tick as appropriate) | | | **Yes** √ | | **No** | |
| **Storage:** | **Maximum amount to be stored on site** | **Secure store out of reach of service**  **users and children** | **Store to be well ventilated** | | **Separate storage facility available or required** | | **Other** |
| (tick all that apply) |  | √ | √ | |  | |  |
| **Method of use.** | **Use undiluted** | **Use diluted** | **Wash hands after use** | | **Do not mix with other products** | | **Special precaution s** |
| (tick all that apply) |  | √ | √ | | √ | |  |
| **State any special/storage requirements or other precautions not listed above:**  Suitable extinguishing media: Not flammable. Use media suitable for surrounding fire | | | | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Type of PPE & Model Nos** | | | **Type of PPE & Model Nos** |
| Safety Glasses EN166 – if risk of splashing | | | Gloves – EN374 Chemical resistant - if prolonged exposure |
| **Who orders PPE?** | **Area Manager** | | |
| **EMERGENCY CONTROLS** | | | |
| **First Aid: Eyes** | | Bathe the eye with running water for 15 minutes. Transfer to hospital for specialist examination. | |
| **Skin** | | Remove all contaminated clothes and footwear immediately unless stuck to skin. Wash immediately with plenty of soap and water. | |
| **Inhalation** | | Remove casualty from exposure ensuring one’s own safety whilst doing so. | |
| **Ingestion** | | Wash out mouth with water. Do not induce vomiting. If Conscious, give half a litre of water to drink immediately. Consult a doctor | |
| **Dealing with spillage:** | | Absorb into dry earth or sand. Transfer to a closable, labelled salvage container for disposal by an appropriate method | |
| **Disposal:** | | Empty containers to be collected as instructed by area manager | |
| **Precautions already in place:** | | PPE, Method statements, Induction and on-going training | |
| **Advice available from?** | | AUTOGLYM | |

2